When are tempering valves needed:
* When a new solid fuel heater with a wet back is fitted.
* A new (not replacement) wet back fitted to an existing solid fuel heater.
* When an additional personal hygiene fixture is installed (i.e. shower unit). In this instance it is only
the new fixture that needs to be tempered but it is easier to temper all the fixtures.
* An owner wants to change the use of an existing building from private dwelling to early child care or retirement home.
* Any new hot water cylinders that supply personal hygiene fixtures or appliances (not direct replacements).
* Bathroom alterations where personal hygiene fixtures are being shifted to new positions.
Please check with your local City Council / Building Authority for final confirmation.
