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	There are probably a lot of practitioners out there that didn’t know that New Zealand Building Code Clause E3 Internal Moisture clause 3.3.3 states with regard to showers:

When enclosures, such as walls, screens, doors or curtains are used they shall be continuous from floor level or top of upstand to 1800 mm minimum above floor level and not less than 300 mm above the shower rose. 
This means the impervious wall i.e. the shower liner must be 300mm above the shower rose. Looking at most off the shelf showers the liners they are only 1800mm high. This places the shower rose at a height of 1500mm unless the liner is extended higher or some other form of impervious surface is used above the shower liner. Apparently, this is because of POSSIBLE splash from the shower rose.


	

		

	

	


